**Groundplex Install for Interworks On <ORG-NAME> Elastic**

**Step One:** Download package

**RPM Installer**

[https://s3.amazonaws.com/elastic.snaplogic.com/snaplogic-sidekick-4.mrc273-x86\_64.rpm](https://s3.amazonaws.com/elastic.snaplogic.com/snaplogic-sidekick-4.mrc260-x86_64.rpm)

**Debian Package**

<https://s3.amazonaws.com/elastic.snaplogic.com/snaplogic-sidekick-4.mrc273-x86_64.deb>

**Windows Zip**

<https://s3.amazonaws.com/elastic.snaplogic.com/snaplex-mrc273.zip>

**Hadooplex binaries**

<https://s3.amazonaws.com/elastic.snaplogic.com/jcc-4.0-mrc273-snapreduce.war>

<https://s3.amazonaws.com/elastic.snaplogic.com/yplex-4.0-snapreduce.jar>

**Step Two:** Install package

Linux platform (x86 64 bit only)

Please make sure rpm and sudo are installed.

Windows platform

Please make sure zip software is installed.

For each platform, follow the installation instruction in URL below:

http://doc.snaplogic.com/#on-premises-snaplex

**Appendix One:** properties for “Org <ORG-NAME>”

1) “**keys.properties**” replace entire file content with the following 4 lines…

**Please note:** The cc.api\_key is one line. Total of 4 lines. Use of text editor such as vi or notepad++ is recommended.

2) “**global.properties**” file update values only with the following...

jcc.subscriber\_id = <ORG-NAME>

jcc.environment = <ENV>